You will need KiCad nightly to open the schematic and PCB files.

hack-the-crab-jtag is the extension board to easily connect two types of
probes to crab. The crab can also be powered from GND/VIN pins on this board, 
when the battery switch is in OFF position (keep the voltage bellow 12V).